If counter value >threshould value IDS Detected

Compare counter and threshould value

Set Timer

Set Counter for that address

Accept Packet And generate MAC

SDN Switch/Router

DFD Level-1 (IDS)